Battery input voltage

14v-16.5v

**PDU**

Servo + proximity sensors circuit

Microcontroller

Pixy camera

14v-16.5v

5V

6V

BLDC Motor Driver

Min 14v

BLDC Motor Driver

Min 14v